IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Description: "ExchangeRequirement[CatalogArticle]"
Time stamp: "2022-09-03T02:09:17"
Preprocessor: "IfcOpenShell 0.5.0-dev"
Originating system: "IfcOpenShell 0.5.0-dev"
Application: "CREATON CAD Bibliothek" version "0.5.0-dev" identifier "CREATON CAD Bibliothek" by Organization "cc" id "cc" description "cc"

People and organizations
  Person "cc" "cc" id "cc" of Organization "cc" id "cc" description "cc"
  Owner history of Person "cc" "cc" id "cc" of Organization "cc" id "cc" description "cc" | application "CREATON CAD Bibliothek" version "0.5.0-dev" identifier "CREATON CAD Bibliothek" by Organization "cc" id "cc" description "cc" | change ADDED | created 1662163757 (2022-09-03T00:09:17Z) | last modified 1662163757 (2022-09-03T00:09:17Z) by Person "cc" "cc" id "cc" of Organization "cc" id "cc" description "cc" with "CREATON CAD Bibliothek" version "0.5.0-dev" identifier "CREATON CAD Bibliothek" by Organization "cc" id "cc" description "cc"

Units
  LENGTHUNIT: MILLI METRE
  PLANEANGLEUNIT: Degrees (conversion based)

Spatial structure
IFCPROJECT
  IFCSITE
    IFCBUILDING
      IFCBUILDINGSTOREY
        contains 1 element
          1 x IFCDISCRETEACCESSORY | names: "Unknown name" | descriptions: "Unknown description" | property sets: Pset_ManufacturerTypeInformation

Property sets
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCDISCRETEACCESSORY)
    Bestellcode Farbe (konkateniert) = "502" (IFCTEXT)
    Bestellcode Farbe = "braun glasiert" (IFCTEXT)
    Bestellcode Farbe Name = "502" (IFCTEXT)
    Bestellcode Funktion = "Flächenziegel" (IFCTEXT)
    Bestellcode Funktion Name = "1000" (IFCTEXT)
    Bestellcode Modell = "FUTURA" (IFCTEXT)
    Bestellcode Modell Name = "610" (IFCTEXT)
    Dachneigung DUO extra (A) = "≥ 17 °" (IFCTEXT)
    Dachneigung DUO extra (D) = "≥ 12 °" (IFCTEXT)
    Dachneigung DUO longlife ND extra (A) = "≥ 17 °" (IFCTEXT)
    Dachneigung DUO longlife ND extra (D) = "≥ 10 °" (IFCTEXT)
    Dachneigung QUATTRO longlife extra (A) = "≥ 15 °" (IFCTEXT)
    Dachneigung QUATTRO longlife extra (D) = "≥ 7 °" (IFCTEXT)
    Dachneigung TRIO extra (A) = "≥ 17 °" (IFCTEXT)
    Dachneigung TRIO extra (D) = "≥ 10 °" (IFCTEXT)
    Deckbreite i.M. (ca.) = "238 mm" (IFCTEXT)
    Deckbreite max. (ca.) = "240 mm" (IFCTEXT)
    Deckbreite min. (ca.) = "235 mm" (IFCTEXT)
    Decklänge i.M. (ca.) = "374 mm" (IFCTEXT)
    Decklänge max. (ca.) = "388 mm" (IFCTEXT)
    Decklänge min. (ca.) = "360 mm" (IFCTEXT)
    Gewicht je Palette (ca.) = "1081 kg" (IFCTEXT)
    Gewicht je Stück (ca.) = "4,3 kg/Stück" (IFCTEXT)
    Gewicht je m² (ca.) = "48,6 kg/m²" (IFCTEXT)
    Größe (ca.) - generiert = "300 x 482 x 76 mm" (IFCTEXT)
    Oberfläche = "FINESSE" (IFCTEXT)
    Produktfamilie = "Flachdachziegel" (IFCTEXT)
    Produktionswerk = "Großengottern" (IFCTEXT)
    Regeldachneigung CREATON AT in Kombination mit Zusatzmaßnahmen nach Herstellerangaben = "17 °" (IFCTEXT)
    Regeldachneigung CREATON CH in Kombination mit Zusatzmaßnahmen nach Herstellerangaben = "18 °" (IFCTEXT)
    Regeldachneigung CREATON DE in Kombination mit Zusatzmaßnahmen nach Herstellerangaben = "14 °" (IFCTEXT)
    UUID = "d156d5a1-ebba-4fec-a89c-536dded7b2de" (IFCTEXT)
    Verpackung (generiert) = "240 Stk./Pal." (IFCTEXT)
    Ziegelbedarf i.M. (ca.) = "11,3 Stück/m²" (IFCTEXT)
    Ziegelbedarf max. (ca.) = "11,9 Stück/m²" (IFCTEXT)
    Ziegelbedarf min. (ca.) = "10,8 Stück/m²" (IFCTEXT)